Router#show running-config

Building configuration...

Current configuration : 1514 bytes

!

! Last configuration change at 02:00:01 UTC Tue Mar 25 2025

!

version 15.4

service timestamps debug datetime msec

service timestamps log datetime msec

no service password-encryption

!

hostname Router

!

boot-start-marker

boot-end-marker

!

!

!

no aaa new-model

mmi polling-interval 60

no mmi auto-configure

no mmi pvc

mmi snmp-timeout 180

!

!

!

!

!

!

!

!

!

!

!

!

ip cef

no ipv6 cef

!

multilink bundle-name authenticated

!

!

!

!

!

!

!

!

!

redundancy

!

!

!

!

!

!

!

!

!

!

!

!

!

!

!

interface Ethernet0/0

ip address 192.168.7.1 255.255.255.0

ip ospf 1 area 0

!

interface Ethernet0/1

ip address 192.168.5.1 255.255.255.0

ip ospf 1 area 0

!

interface Ethernet0/2

no ip address

ip ospf 1 area 0

shutdown

!

interface Ethernet0/3

ip address 192.168.8.1 255.255.255.0

ip ospf 1 area 0

!

interface Ethernet1/0

ip address 192.168.107.150 255.255.255.0

!

interface Ethernet1/1

no ip address

shutdown

!

interface Ethernet1/2

no ip address

shutdown

!

interface Ethernet1/3

no ip address

shutdown

!

router ospf 1

network 192.168.5.0 0.0.0.255 area 0

network 192.168.7.0 0.0.0.255 area 0

network 192.168.8.0 0.0.0.255 area 0

!

ip forward-protocol nd

!

!

no ip http server

no ip http secure-server

ip route 0.0.0.0 0.0.0.0 192.168.107.2

ip route 192.168.3.0 255.255.255.0 192.168.7.2

ip route 192.168.3.0 255.255.255.0 192.168.8.2

ip route 192.168.6.0 255.255.255.0 192.168.5.2

!

!

!

!

control-plane

!

!

!

!

!

!

!

!

line con 0

logging synchronous

line aux 0

line vty 0 4

login

transport input none

!

!

end